The coordinate point provided in the marine licence application marks the end of the outfall pipe.

The coordinate point where the route of the buried pipe bisects the MHWS is at X (Easting) 444789, Y (Northing) 1153703.  For latitude and longitude, this is 60.265091 North, 1.1923472 West.