Appendix C – Continuation from Question 6 Deposits and Removals

When re-stacking existing concrete interlocking blocks, it may be necessary first (depending on subgrade to lay an appox 200mm thick surface regulating layer of bituminous macadam. This would be below MHWS but would be laid during low tide conditions preventing any material escaping into the watercourse. The material would be set and cooled well before contact with water on the rising tide and would be concealed within the rock revetment.

Volume – approximately 1-2m3.

Weight- Approx 2.2 – 4.4 tonnes

Area approx. 10m2